en

conf t

hostname MSW2

int vlan 1

ip address 192.168.20.2 255.255.255.0

no shutdown

exit

ip default-gateway 192.168.20.1

enable secret c1sc0

line console 0

password c0ns0l3

exit

service password-encryption

ip domain-name cisco.com

crypto key generate rsa

1024

username sarah password p4ssw0rd

line vty 0 4

login local

transport input ssh

end

copy run start